# Supported Systems and Drivers

Mesa was originally designed for Unix/X11 systems and is still best supported on those systems. All you need is an ANSI C compiler and the X development environment to use Mesa.

The DRI hardware drivers for the X.org server and XFree86 provide hardware accelerated rendering for chips from ATI, Intel, Matrox, 3dfx and others on Linux and FreeBSD.

Drivers for other assorted platforms include: the Amiga, Apple Macintosh, BeOS, NeXT, OS/2, MS-DOS, VMS, Windows 9x/NT, and Direct3D.

Details about particular drivers follows. Be warned that some drivers may be out of date and no longer function.

- Xlib driver for the X Window System
- DRI hardware drivers for the X window system
- Microsoft Windows (README.WIN32)
- DEC VMS (README.VMS)
- 3dfx/Glide (README.3DFX)
- GGI (README.GGI)
- Amiga Amiwin (README.AMIWIN)
- BeOS (README.BEOS)
- Direct3D driver (README.D3D)
- DJGPP (README.DJ)
- LynxOS (README.LYNXOS)
- Mingw32 (README.MINGW32)
- NeXT (README.NeXT)
- OpenStep (README.OpenStep)
- OS/2 (README.OS2)
- WindML (README.WINDML)
- Utah GLX drivers